# Product Specification

1. Number of Fingerprints stored simultaneously for direct keypad location: 15.
2. Maximum fingerprint memory capacity 162 Fingerprints.
3. Times

|  |  |
| --- | --- |
| Action 1 | 1 |
| 2 | <2 from Keypad input |
| 3 | <4 to Display outcome, from pin selection |
| 4 | <2 |
| 5 | 1 |
| 6 | 0.5 |

1. 5V DC
2. FRR 10% for Thumb Index and Third finger
3. FFR 35% for 4th and 5th finger
4. Scanner requires the User to be set up as an administrator by a technician to access admin features.